**7S**

# TEMPORARY INFORMATION SIGNING

(Effective September 24, 2013; Revised July 31, 2020)

**Description**. This work shall consist of the furnishing, installation, maintenance, and removal of temporary information signs.

**Materials**. Materials shall be according to the applicable portions of Section 701 of the Standard Specifications and as shown on the plans.

**Construction Requirements**. The temporary information signs shall be in place at least one week prior to the beginning of construction activities that impact traffic flow and shall remain in place until the completion of the project. If all lanes are open for an extended period of time during the project, the Contractor shall cover the signs until lane closures resume. If the project is shut down for the winter, the signs shall read “Road Work Resumes Spring XXXX.”

Signs shall be installed according to the requirements of Section 701.

**Method of Measurement**. This work will be measured for payment in square feet in place. The auxiliary sign panel will not be measured for payment.

**Basis of Payment**. This work will be paid for at the contract unit price per square foot for TEMPORARY INFORMATION SIGNING.

DESIGNER NOTES:

Do not include on projects when additional changeable message boards are to be used.

Include CADD detail 720-8, 720-9, 720-10 or 720-11 in the plans.

Include pay item for Z0030850 TEMPORARY INFORMATION SIGNING.

720-8: To be used on all contracts when designated in the TMP or when closing a lane in the construction zone for five or more calendar days and no correspondence was required or completed with local officials.

720-9: To be used on all contracts when designated in the TMP or when a detour is required for traffic.

720-10: To be used on all contracts when designated in the TMP or when closing the road to traffic.

720-11: To be used on all contracts when designated in the TMP or when closing the road to thru traffic.