## PORTLAND CEMENT CONCRETE SIDEWALK 5 INCH, SPECIAL

Revised 07/06/23

This work shall include all materials, labor, and equipment necessary to construct the portland cement concrete sidewalk, excavation, grading, and seeding and mulch at locations shown on the plans and as directed by the Engineer.

This work shall be in accordance with Section 424.

The excavation necessary for construction of the portland cement concrete sidewalk shall be included in contract unit price and in accordance with Section 202.

After the approved backfill is complete per Article 424.10, the Contractor shall prepare the seed bed, apply fertilizer, and Class 1 seed mixture in accordance with Section 250.  Mulch, Method 1 shall be placed on the seeded areas in accordance with Section 251.

Basis of Payment.  This work will be paid for at the contract unit price per square foot for PORTLAND CEMENT CONCRETE SIDEWALK 5 INCH, SPECIAL.  Price shall include all earth excavation, fertilizing, seeding and mulch.