**2A**

# EXCAVATING AND GRADING EXISTING SHOULDER

(Effective: November 26, 2013)

This work shall proceed according to Section 202 of the Standard Specifications. All excavated material shall be placed on the foreslope, adjacent to the proposed HMA shoulder. The material shall be compacted to the satisfaction of the Engineer. The area shall then be seeded, fertilized, and mulched. The Contractor shall not remove any excavated material from the project limits.

This work, including the placing and compacting material, will be paid for at the contract unit price per unit for EXCAVATING AND GRADING EXISTING SHOULDER. Seeding, fertilizer and mulch will be paid for separately.

DESIGNER NOTE:

To be used on projects lacking environmental clearance, where removal of excavated material from the jobsite is prohibited.