# 4O

# RUMBLE STRIPS AT INTERSECTIONS

(Effective April 17, 2001; Revised February 18, 2009)

**Description**. This work shall consist of constructing rumble strips in the pavement at the locations shown on the plans.

**Construction Requirements**. This work shall be done according to the applicable portions of Section 642 of the Standard Specifications and the details on the plans.

**Method of Measurement.** Rumble strips will be measured as each, where each is defined as a 25 ft length installation.

**Basis of Payment.** This work will be paid for at the contract unit price each for RUMBLE STRIP.

DESIGNER NOTE: Include CADD Detail 440-3 for Rumble Strip in the plans.