**7AG**

# MODIFIED URETHANE PAVEMENT MARKING – TWO APPLICATIONS

(Effective March 30, 2023)

**Description**. This work consists of furnishing and applying modified urethane pavement marking according to Section 780 of the Standard Specifications except that the modified urethane shall be applied in two applications.

**Materials**. Each application shall meet the requirements of Article 780.12 of the Standard Specifications.

**Construction Requirements**

**General.** The first application shall be allowed to cure for a minimum of 14 days prior to placing the second application over the first. The Contractor shall not place one thick application in lieu of two regular applications.

**Basis of Payment**. Each application will be measured and paid for.