# AGGREGATE BASE COURSE

Eff. 09-11-1990 Rev. 01-01-2014

In addition to the requirements of Section 351 of the Standard Specifications, the aggregate base course shall be placed in at least two lifts and the final 4-inch (100 mm) (compacted) layer of aggregate shall be deposited full-lane width with a spreading and finishing machine meeting the requirements of Article 1102.03 of the Standard Specifications. The spreading and finishing machine shall be equipped with a leveling device as specified in Article 1102.03.

Any cost incurred due to the required two lifts and use of the spreading and finishing machine on the final 4-inch (100 mm) layer of aggregate will not be paid for separately, but shall be included in the contract unit price for AGGREGATE BASE COURSE of the type specified.