# NEW DOMESTIC SANITARY SERVICE

Eff. 09-11-1990 Rev. 01-01-2014

At locations as directed by the Engineer or City of XXXXX, new domestic sanitary sewer lines shall be constructed from the existing 8 inch, 10 inch, 12 inch (200 mm, 250 mm, 300 mm) sanitary sewers to the right-of-way lines.

This work shall be in accordance with the City of XXXXX Standard Specifications for Sanitary Sewers and is to be accomplished without interruption of flow in the sanitary sewers.

Estimated quantities have been included in this section for TAPPING SADDLE 6 in (150 mm) and SANITARY SEWER, TYPE 2, 6 in (150 mm) and it is hereby understood and agreed that should the Engineer delete all or any part of these items, the Contractor will receive no remuneration for the deleted item.

This work shall be paid for at the contract unit price each for TAPPING SADDLE, 6 in (150 mm) which price shall include the cost of making the tap, making all connections, and all joint materials. The sewer line will be paid for at the contract unit price per lineal foot (meter) for SANITARY SEWER of the type and size specified which price shall include the cost of all excavation, except excavation in rock, and backfilling. Trench backfill shall be measured and paid for as provided in Section 208 of the Standard Specifications.