**7AE**

# PAINT PAVEMENT MARKING – TWO APPLICATIONS

(Effective: November 1, 2011)

**Description**. This work consists of furnishing and applying paint pavement marking according to Section 780 of the Standard Specifications except that the paint shall be applied in two applications.

**Materials**. Each application shall meet the requirements of Article 780.06 of the Standard Specifications.

**General**. The first application shall be allowed to dry prior to placing the second application over the first. The Contractor shall not place one thick application in lieu of two regular applications.

**Basis of Payment**. Each application will be measured and paid for.