# 4P

# RAISED JOINT REMOVAL

(Effective November 1, 1992); Revised January 1, 2007)

This work shall consist of the satisfactory removal and disposal of HMA material along a transverse pavement joint that has been identified as a high area. This work shall be done prior to placing the proposed HMA resurfacing.

The work shall be accomplished in a manner that does not damage the portions of the existing roadway that will remain. The high area will be removed to a tolerance of 1/4 in. or less when checked with a 10 ft. straightedge referenced to adjacent pavement.

Raised joint removal will be measured as each, where each is per joint per lane.

This work will be paid for at the contract unit price each for RAISED JOINT REMOVAL.