# MASTIC REPAIRS FOR CULVERTS

**Description.** This work shall include cleaning and sealing joints and weep holes of existing culverts with mastic at locations specified in the plans.

**Materials.** Mastic shall be according to Section 1055 of the Standard Specifications.

**Construction Requirements**. The existing joints or weep holes shall be cleaned of any loose debris, unsound or any other foreign materials using methods approved by the Engineer.  The crack or weep holes shall then be filled with mastic.

**Method of Measurement.** This work will be measured for payment on a lump sum basis.

**Basis of Payment**. This work will be paid for at the contract lump sum price for MASTIC REPAIRS FOR CULVERTS.

*Designer notes: can be used for sealing joints on pipe as well as plugging weep holes.*