# 7AL

# TEMPORARY RUMBLE STRIPS (SPECIAL)

(Effective March 30, 2023)

**Description**. This work shall consist of the furnishing, installation, maintenance, and removal of temporary rumble strips and advance signage.

**Materials**. Materials shall be according to the following:

Item Article/Section

(a) Sign Posts, Metal (Note 1) 1093.01(a)

(b) Sign Posts, Wood (Note 2) 1007.05

(c) Preformed Plastic Pavement Markings 780.07

Note 1. Galvanizing of metal posts will not be required.

Note 2. The nominal size of wood posts shall be 4 in x 4 in.

**Equipment**. Equipment shall be according to the following:

Item Article/Section

(a) Signs 1106.01

**CONSTRUCTION REQUIREMENTS**

**General**. The rumble strips shall consist of six layers of Preformed Plastic Pavement Marking, Type B - Inlaid - Line 6" (White). The temporary rumble strips shall be placed as shown in the plans or as directed by the Engineer.

Advance signage shall be furnished and installed as shown on the applicable plan details.

**Method of Measurement**. This work will be measured for payment as each, where each is defined as a set of three temporary rumble strips across a single lane of pavement

**Basis of Payment**. This work will be paid for at the contract unit price per each for TEMPORARY RUMBLE STRIPS (SPECIAL).