# STEEL PLATE BEAM GUARDRAIL (SHORT RADIUS)

Eff. 01-01-2024

This work shall consist of furnishing and erecting steel plate beam guardrail at the radius specified at the location shown in the plans.

This work shall be in accordance with Section 630 of the Standard Specifications and as shown on the plans. The guardrail shall conform to Steel Plate Beam Guardrail, Type A.

The Contractor shall provide shop drawings to verify the connections between elements and ability to construct the guardrail in the specified location.

Method of Measurement.This work will be measured for payment in feet along the top edge of the rail elements, continuous through laps and splices.

Basis of Payment. This work will be paid for at the contract unit price per foot of STEEL PLATE BEAM GUARDRAIL (SHORT RADIUS).