Regional Engineers

Maureen M. Addis

Special Provision for Hot-Mix Asphalt – Tack Coat

July 22, 2016

This special provision was developed by the Bureau of Materials and Physical Research in response to District requests for a quicker setting tack coat for night-time paving or other paving conditions that are not ideal for traditional setting tack coats.

This special provision should be inserted into all HMA paving contracts.

The districts should include the BDE Check Sheet marked with the applicable special provisions for the November 4, 2016 and subsequent lettings. The Project Coordination and Implementation Section will include a copy in the contract.

This special provision will be available on the transfer directory July 22, 2016.

80376m

# hot-mix asphalt – tack coat (bde)

Effective: November 1, 2016

Revise Article 1032.06(a) of the Standard Specifications to read:

“(a) Anionic Emulsified Asphalt. Anionic emulsified asphalts shall be according to AASHTO M 140. SS-1h emulsions used as a tack coat shall have the cement mixing test waived.”

80376