**6L**

# **CONCRETE HEADWALLS FOR PIPE DRAIN (SPECIAL)**

(Effective January 1, 2026)

This work shall consist of constructing underdrain outlet protectors in accordance with the details shown on the plans and Article 601.05 of the Standard Specifications.

**Basis of Payment.**  Concrete headwalls for pipe drain (special) will be paid for at the contract unit price per each for CONCRETE HEADWALLS FOR PIPE DRAIN (SPECIAL).

Designer Note:

This should be used on Interstate reconstruction projects. When this special provision and associated detail is used, the precast outlet (Highway Standard 601101) is not used.

District 3 Detail 601-7 must be included when this special provision is used.

Temporary pay item number will be #3003080