# OPENING LANES FOR UNVIVERSITY OF ILLINOIS MOVE-IN DAYS

Eff. 01-01-2024

No broken pavement, open holes, trenches, barricades, cones, or drums will remain on or adjacent to the traveled way and all lanes shall be opened to traffic during U of I Move-in days, except where major bridge construction and/or other roadway reconstruction (excluding patching and resurfacing) requiring overnight lane closures would make it impractical. Only the general move-in day is restricted. The Contractor will have to coordinate with the Engineer to obtain these dates.  These requirements shall apply in addition to any other requirements in the Standard Specifications