**PIPE UNDERDRAINS TYPE 2, 4 INCH**

Revised 2/10/17

This work shall be according to Section 601 of the Standard Specifications and Standard 601001, except the perforated pipe shall be encased in fabric in accordance with article 1080.01.

**Designer Notes:**

**To be used on all projects with Pipe Underdrains**.