**7B**

# WIDTH RESTRICTION SIGN

(Effective April 24, 2017)

Width restriction signs, as shown in Standard 701901 – Traffic Control Devices, shall be used on this project. They shall be placed as follows:

|  |  |  |
| --- | --- | --- |
| **MAX WIDTH** | **MILES AHEAD** | **SIGN LOCATION**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

The cost of supplying, installing, maintaining, and removing width restriction signs shall be included in the cost of the traffic control and protection pay items.

*Designer Note: Fill in the maximum width, miles ahead and location for all signs as shown in the example below. If the widths change for different stages, this should also be specified.*

|  |  |  |
| --- | --- | --- |
| ***MAX WIDTH*** | ***MILES AHEAD*** | ***SIGN LOCATION***  |
| *10’-6”* | *10 MILES AHEAD* | *NB on north leg of IL 47 & IL 116* |
| *10’-6”* | *3-1/2 MILES AHEAD* | *SB on south leg of IL 47 & IL 17* |
|  |  |  |
|  |  |  |

 *When an actual width of 13’-6” or less is proposed, the width restriction sign will show the opening to be 18 inches less than the actual width. Openings greater than 13’-6” will not require a restriction sign.*