# EXCAVATION

Eff. 09-11-1990 Rev. 01-01-2014

Excavation adjacent to the existing pavement remaining open during non-working hours shall not exceed XXXXX needed for filling the trench with XXXXX.

No additional compensation will be allowed the Contractor for compliance with the requirements of this Special Provision.

*PROGRAM DEVELOPMENT NOTES - Determine maximum length of excavation ahead of shoulder, widening, etc. and whether it may be left open at night or whether it must be filled each day. This is to be done during preparation of the Traffic Control Plan. Also this special provision must be coordinated with the pay item for 'EXCAVATING AND GRADING EXISTING SHOULDER,' if used.*

(Program Development Notes shall not appear in the Special Provision.)